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FORMULAR DE LICITAȚIE – APROVIZIONARE (ST5)

privind achiziționarea soluției camere de corp (Bodycam) în cadrul proiectului de asistență externă ,,Gestionarea eficientă a procesului de migrare într-un context transfrontalier” PRO GOV, ROMD00131

Finanțat prin programul INTERREG NEXT VI-A 

România – Republica Moldova 2021 – 2027
1. INFORMAȚII DESPRE OFERTĂ

	Trimis de: 
	Nume(e) și adresă(e) entității sau entităților juridice care depun această licitație

	Îngrijirea
	

	Reprezentant legal
	

	TVA/număr de înregistrare

	

	Naționalitate

	

	Adresă
	

	Telefon 
	

	E-mail
	

	Persoană de contact
	

	Date bancare
	Numele contului bancar: 
Numărul contului bancar: 
Nume al băncii: 
Cod SWIFT: 
IBAN: 

	Numărul lotului

	


2. DECLARAȚIA OFERTANTULUI 
Eu, semnatul menționat, confirm că materialele oferite în această procedură de achiziție sunt în deplină conformitate cu specificațiile prezentate de autoritatea contractantă. Descrierea detaliată a proviziilor oferite de noi este oferită în următorul punct. 

În plus, confirmăm că organizația/compania noastră este pe deplin eligibilă pentru livrarea de materiale în baza unui contract finanțat de fondurile UE. Confirmăm că nu ne aflăm în niciuna dintre situațiile care ne-ar exclude de la concurența în procedurile de achiziții finanțate de UE, așa cum este indicat în [punctul 18 din Anexa II a Acordului de Finanțare dintre Comisia Europeană și țara parteneră
][punctul 18 din Anexa I a Regulamentului 2018/1046
]. De asemenea, confirmăm că nu avem niciun conflict de interese cu vreun membru al autorității de contractare sau cu alți ofertanți.

Eu, semnatarul, declar că domeniul nostru de activitate este pe deplin în conformitate cu subiectul actualei proceduri de licitație.

Eu, subsemnat, declar, de asemenea, că, în legătură cu procedura actuală de licitație, nu ne aflăm în situație, încercând să influențăm în mod nejustificat procedura de acordare sau să obținem informații confidențiale, deoarece acestea ar trebui tratate ca o abatere profesională gravă, ceea ce poate duce la respingerea procedurii de acordare.

[Declarația privind onoarea privind criteriile de excludere și criteriile de selecție este atașată.]

[Dovezile (documente justificative) pentru criteriile de selecție vor fi depuse la solicitare.]

	Nume
	

	Semnătură
	

	Data
	


3. CRITERII DE EXCLUDERE ȘI SELECȚIE
Criteriile de excludere și selecție aplicabile prezentei proceduri sunt cele prevăzute în Invitația de participare și Caietul de sarcini.

Ofertantul declară că îndeplinește integral toate cerințele stabilite de autoritatea contractantă.

4. OFERTĂ TEHNICĂ ȘI FINANCIARĂ

Ofertanții sunt obligați să ofere o ofertă tehnică, pe baza cerințelor indicate de autoritatea contractantă în Invitația la licitație, Informații tehnice. Ofertanții vor furniza prețurile tuturor articolelor și detalii despre livrarea planificată a materialelor, inclusiv specificații detaliate.
	Nr. d/o
	Numărul de obiecte
	Titlul articolului
	Ofertă tehnică
	Ofertă financiară

	
	
	
	Elemente oferite de ofertant, pe baza cerințelor și informațiilor
(marca și numele concret vor fi indicate aici)
	Preț 

(lei, MD/EURO buc.)
	SUMA totală
(lei, MD/EURO)

	(menționarea numelor de mărci este permisă doar dacă opțiunea "sau echivalentul" este disponibilă, permițând oferirea altor branduri)

	Soluție camere de corp (Bodycam)

	1.
	30 
	Body-worn camera / VB-440-64-KF-N
	Dimensions

Maximum H 100 mm x W 80 mm x D 30 mm

Weight

Maximum 200 g (excluding mountings)

Battery

Li-Ion / Li-Pol

Battery run time

More than 12 hours video recording @ 720p

Battery recharging time

Typically recharges in less than 8 hours

Storage capacity

Minimum 64 GB, encrypted AES 256

Image sensor

CMOS

Image sensor sensitivity

Better than 0.2 lux

Lens capture angle

Horizontal: min 120°, Vertical: min 60°

Video compression

At least H.264

Video resolutions

1920x1080 and 1280x720

Video framerate

25 fps / 30 fps

Pre / post-record

Up to 2-minute pre / post-recording buffer

Audio compression

AAC or MP3

Audio bitrate

128 kbps

Connectivity

Wi-Fi 802.11 a/b/g/n, Bluetooth

Notifications

Audible, visual or vibration notifications

Casing

At least IP67 rated, drop tested up to 1.8 m

Operating temperature

At least -20°C to +50°C

Security features

Restriction on viewing, downloading, or deletion of any recordings directly from the camera

Fixings

Klick Fast, with quick-release stud chest harness (KF-HARN4)

Warranty

At least 2 years, with the possibility of extension

User Manual

English & Romanian versions (hardcopy or electronic)


	
	

	2.
	30 
	Licență Bodycamere / VM-EPL-VB-PLUS-1
	Purpose

Per-camera software licence required to enable each proposed body-worn camera to operate with the centralized VideoManager platform

License type

On-premises per-device licence for body-worn cameras

Licensing scope

One licence for each proposed body-worn camera

Functions

Body-worn camera management, user and role management, incident / evidence handling, search, filtering, viewing, export, audit support, media import, reporting and interface customisation

Streaming

Support for live streaming from body-worn cameras to VideoManager over Wi-Fi and serving streams / recordings to an ONVIF-compatible VMS

Compatibility

Compatible with the proposed VB400 body-worn cameras and with the proposed centralized VideoManager / HQ management platform

Software assurance

Minimum 12 months Software Assurance included, with the possibility of extension

License model

Perpetual on-premises licence or equivalent commercial model offered by the manufacturer


	
	

	3.
	3
	Stații de andocare pentru Bodycamere / VB-400-DOCK14/EU
	Purpose

Simultaneous charging, configuration and video offload/download for body-worn cameras after the working shift

Docking ports quantity

14-port dock; minimum 10 charging positions per location, as applicable, through one or more docking stations

Docking cameras

The camera shall fit into the docking slot without removal of wearable fixings or attached compatible accessories

Power input

Supplied power adapter, input 100–240 V AC, 50/60 Hz; dock power requirement 12V / 5A

Connectivity

USB connection to DockController / controller; USB 2.0 and USB 3.0 compatible

Compatibility

Compatible with proposed VB400 body-worn cameras and DockController DC-200 / management platform

Mounting

Suitable for desk, shelf or secure mounting surface installation

Operating temperature

Indoor use; charger ambient temperature shall not exceed +40°C

Warranty

Minimum 2 years supplier warranty; extended warranty availability

User Manual

User manual / quick start documentation in English; Romanian version to be provided by the supplier


	
	

	4.
	1
	Platformă software centralizată pentru administrarea și gestionarea înregistrărilor provenite de la bodycamere / VM-EPL-HQ-BASE sau echivalent (Soluție de stocare a informației de pe Bodycamere)
	Purpose

Centralized administration of cameras, users, licenses, recordings and access rights
Functions

Upload, storage management, search, filtering, viewing, export, audit trail and access control

Compatibility

Compatible with proposed body-worn cameras, docking stations, controller and RFID equipment

License model

Base license + per-camera PLUS licenses


	
	

	5.
	30
	Suport magnetic pentru Bodycamere / KF-MAGMOUNT2
	Purpose

Secure attachment of the body-worn camera to uniform or clothing

Mount type

Heavy-duty magnetic Klick Fast mounting set, supplied with magnets

Compatibility

Compatible with the proposed VB400 body-worn cameras with Klick Fast fixing

Fixing method

Powerful magnetic backing plate for secure positioning on clothing during the working shift

Installation

No tools required for normal use; quick mounting and removal

Material / construction

Durable mounting accessory suitable for daily operational use

Warranty

Minimum 24 months supplier warranty


	
	

	6.
	1
	Cititor pentru Bodycamere / RF-220
	Purpose

Rapid allocation / assignment of body-worn cameras to users by means of existing ID or access cards

Product Code

RF-220 or equivalent

Typical Usage

Attached to a DC-200 via USB connection

Management Software

Video Manager 9.1 onwards (for High & Low frequency card support) BT/NFC may be supported in a future Video Manager release

Frequency

Low Frequency: 134.2 kHz

High Frequency: 13.56 MHz

Read / Write Distance

Low Frequency and High Frequency: 4 in (100 mm)

Supported Compatible Card Standards

Including but not limited to: ISO/IEC 14443 Type A, ISO/IEC 14443 Type B, ISO/IEC 15693; including compatibility with existing access / identification cards where applicable

Operating Temperature

0° to 40°C

Storage Temperature

-55° to 70°C

Warranty

Minimum 24 months supplier warranty

Dimensions

Approx. 88 x 56 x 18 mm


	
	

	7.
	1
	DockController Bodycamere
	Purpose

Aggregates multiple body-worn camera docks and transfers footage / metadata from body-worn cameras to the centralized VideoManager platform; enables rapid camera assignment to users via RFID where required

Product Code

DC-200/EU or equivalent

Typical Usage

Connected to VideoManager over Ethernet, with multiple docks attached via USB

Camera Capacity

Support for up to 84 body-worn cameras per DockController

RFID

Compatible with external RFID reader for user-to-camera assignment, e.g. RF-220, connected via USB

Connectivity

USB connection to docking stations; Ethernet 1000Base-T to external network

Power input

Supplied external power supply, input 100–240V AC, 47–63 Hz

Operating temperature

0°C to +40°C

Warranty

Minimum 24 months supplier warranty

User Manual

English & Romanian versions (hardcopy or electronic)


	
	

	8.
	1
	Dispozitiv local de stocare pentru Bodycamere / NVR6-PRM-FORM-D-96TB-S22
	Purpose

Local on-premises storage server for secure storage and management of body-worn camera recordings, integrated with the proposed centralized management platform and, where applicable, with Avigilon Unity Video / ONVIF-compatible VMS environments.

Form factor

2U rack-mount chassis.

Effective storage capacity

Minimum 96 TB usable storage.

Raw storage capacity

Minimum 120 TB raw storage.

RAID configuration

RAID 6 for video data storage

Operating system

Microsoft Windows Server 2022 LTSC, factory installed.

System disk configuration

2 × 480 GB M.2 SSD, RAID 1, for operating system.

Storage drive configuration

Up to 12 × 3.5" hot-swappable SATA drives.

Network interfaces

6 × 1 GbE RJ-45 ports and 4 × 10 GbE SFP+ ports.

Cybersecurity

Built-in TPM 2.0 supporting hardware Root of Trust authentication and data encryption.

Power input

100 to 240 VAC, 50/60 Hz, auto-switching

Power supply

Dual redundant (1+1) 1400 W hot-swappable power supplies.

Operating temperature

10°C to +35°C.

Storage temperature

-40°C to +65°C.

Dimensions

Approx. 721.6 × 482.0 × 86.8 mm.

Included UPS

Eaton 9E3000IR UPS, 3000 VA, 2700 W, Rack, 2U, USB, 6 × C13 and 1 × C19 outputs, or equivalent

UPS topology

Online / double-conversion

UPS communication

USB and RS232

UPS operating temperature

0°C to +40°C

Warranty

5-year 4-hour mission-critical warranty with onsite parts delivery service, or equivalent.


	
	

	9.
	1
	Stație centrală de monitorizare și stocare locală pentru Bodycamere (Dispozitiv central de stocare a info pentru Bodycamere)
	Purpose

Central local workstation for viewing, playback and local recording/storage of body-worn camera video within the proposed integrated video management architecture

Product Code

NVR5-WKS-8TB-EU or equivalent

System type

All-in-one network video recorder and client workstation

Storage capacity

Minimum 8 TB local video data storage

Use case

Suitable for small to medium sites requiring local recording and playback

Recording throughput

Up to 120 Mbps recording data rate

Playback / live streaming

Up to 100 Mbps

Operating system

Microsoft Windows 10 IoT Enterprise LTSC (2021) or equivalent

Processor

Intel Core i3, 12th generation or equivalent

Memory

Minimum 8 GB DDR4 RAM

OS drive

Minimum 256 GB SSD

Network interface

2 × 1 Gigabit Ethernet RJ-45 ports

Monitor interfaces

Up to 2 monitors via DP / HDMI combination

Power input

90 to 264 VAC, 50/60 Hz, auto-switching

Power supply

Single PSU

Operating temperature

+5°C to +45°C

Storage temperature

-40°C to +70°C


	
	

	10.
	1
	Camere video de supraveghere / 2.0C-H6A-D1-IR sau echivalent, cu injector PoE+ 30W inclus
	Purpose

Indoor fixed dome IP camera for video surveillance in the body-worn camera management / evidence handling environment, including overview of operator / storage / control areas

Camera type

Indoor IR dome camera

Resolution

Minimum 2 MP

Lens

Varifocal 2.8–12 mm

IR illumination

Integrated IR illumination

Analytics

Built-in video analytics; audio analytics where supported by H6A model

Audio

Built-in microphone, where supported by the proposed H6A model

Image compression

H.264 HDSM SmartCodec, H.265 HDSM SmartCodec, Motion JPEG

Network

RJ-45 Ethernet connection; 100BASE-TX

ONVIF

ONVIF Profile S, T, M and G compliant

Local storage

Support for onboard microSD / microSDHC / microSDXC storage

Power

PoE IEEE 802.3af Class 3 and PoE+ IEEE 802.3at Class 4; max. power consumption up to 25 W

Injector

Supplied with 1-port PoE+ injector, minimum 30 W, with European power cord

Operating temperature

-10°C to +55°C

Protection

Minimum IP54; vandal resistance up to IK10 for IR surface mount indoor version

Compatibility

Compatible with the proposed Avigilon / Motorola video management architecture

Warranty

Minimum 3 years manufacturer warranty or better


	
	

	
	
	Termen de livrare: 31.07.2026.

Locul livrării: Inspectoratul General de Carabinieri, str. Gheorghe Asachi 65A, MD-2028, Chișinău, Republica Moldova
Perioada de garanție: minimum 24 luni de la semnarea documentelor de recepție și/sau de la data punerii în funcțiune și acceptanța finală. Furnizorul va asigura intervenția în termen de maximum 48 de ore de la notificarea defecțiunii și remedierea acesteia fără costuri suplimentare pentru Beneficiar.
	
	

	TOTAL:
	


Prețurile sunt exprimate în:

· MDL - pentru operatorii economici rezidenți;

· EURO - pentru operatorii economici nerezidenți.

Dacă oferta include valori exprimate în altă monedă, conversia se va realiza conform cursului InforEuro aferent lunilor aprilie 2026 (publicat la: https://ec.europa.eu/budget/graphs/inforeuro.html). 

Evaluarea ofertelor financiare se va efectua în valuta națională MDL, cu aplicarea cursului InforEuro la data depunerii ofertei, în cazul în care vom avea oferte depuse în diferite valuate, MDL sau EURO.
Prețul include toate costurile aferente furnizării bunurilor: personalizare, ambalare, transport și livrare la sediul autorității contractante.
Conform legislației fiscale aplicabile din Republica Moldova, inclusiv prevederile Hotărîrii Guvernului Republicii Moldova nr. 246/2010 cu privire la modul de aplicare a facilităților fiscale şi vamale aferente realizării proiectelor de asistență tehnică şi investițională în derulare, care cad sub incidența tratatelor internaționale la care Republica Moldova este parte sau a contractelor de stat, cu modificările ulterioare, proiectul sus menționat se regăsește în Anexa nr. 1 a Hotărârii prenotate, care stabilește Lista proiectelor de asistență tehnică în derulare, care cad sub incidența tratatelor internaționale, pentru aplicarea scutirilor la impozitul pe venit, accize, taxe vamale, taxe pentru efectuarea procedurilor vamale, taxe pentru mărfurile care, în procesul utilizării, cauzează poluarea mediului, precum şi aplicarea scutirii de TVA cu drept de deducere pentru mărfurile şi serviciile destinate acestora.
Prețul oferit include livrarea articolelor descrise, precum și toate costurile aferente (de exemplu transport, logistică, costuri materiale) atunci când este necesar. 

	Numele semnatarului autorizat
	

	Semnătură
	

	Data
	


� Unde este cazul. Pentru indivizi, menționează cartea de identitate, pașaportul sau un document echivalent – numărul.


� Conform formularului de entitate juridică și documentelor justificative atașate.


� Unde este cazul. În cazul mai multor loturi, oferta tehnică și financiară va fi prezentată pentru fiecare lot.


� Pentru partenerii aflați în țările partenere.


� Pentru partenerii aflați în statele membre, care nu sunt autorități contractante în sensul legislației Uniunii aplicabile procedurilor de achiziții publice.
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